### AX6 Setup

In OMGUI (https://github.com/digitalinteraction/openmovement/wiki/AX3-GUI), set the following options:

[Tools][Options] set [Filename] = {SubjectCode}\_{DeviceId}

[File][Choose Working Folder] = set to Z:\Axivity\cwa\_files\

To program device – [clear][record]

Recording Settings

[Sampling] = 12.5Hz

[Recording Time][Range] = +/- 8g

[Interval = anticipated wear start time +24h

[Subject][Code] = “studyID”

Untick [Flash during Recording]

[Lower power]

[Unpacked data]